/*
 * Copyright (c) 2020-2024, Arm Limited. All rights reserved.
 *
 * SPDX-License-Identifier: BSD-3-Clause
 */

/dts-v1/;

#define	AFF	00

#include "fvp-defs.dtsi"
#undef POST
#define	POST \
	};

/ {
	compatible = "arm,ffa-core-manifest-1.0";
	#address-cells = <2>;
	#size-cells = <2>;

	attribute {
		spmc_id = <0x8000>;
		maj_ver = <0x1>;
		min_ver = <0x2>;
		exec_state = <0x0>;
		load_address = <0x0 0x6000000>;
		entrypoint = <0x0 0x6000000>;
		binary_size = <0x80000>;
	};

	hypervisor {
		compatible = "hafnium,hafnium";
		vm1 {
			is_ffa_partition;
			debug_name = "op-tee";
			load_address = <0x6280000>;
			vcpu_count = <8>;
			mem_size = <0xd80000>;
		};
	};

	cpus {
		#address-cells = <0x2>;
		#size-cells = <0x0>;

		CPU_0

		/*
		 * SPMC (Hafnium) requires secondary core nodes are declared
		 * in descending order.
		 */
		CPU_7
		CPU_6
		CPU_5
		CPU_4
		CPU_3
		CPU_2
		CPU_1
	};

	memory@6000000 {
		device_type = "memory";
		reg = <0x0 0x6000000 0x0 0x2000000>; /* Trusted DRAM */
	};

	memory@80000000 {
		device_type = "ns-memory";
		reg = <0x0 0x80000000 0x0 0x7c000000>,
		      <0x8 0x80000000 0x1 0x80000000>,
		      <0x00008800 0x80000000 0x0 0x7f000000>;
	};

	memory@0 {
		device_type = "device-memory";
		reg = <0x0 0x1c090000 0x0 0x40000>; /* UART */
	};
};
