/*
 * Copyright (c) 2020, Arm Limited. All rights reserved.
 *
 * SPDX-License-Identifier: BSD-3-Clause
 *
 * This file is a Partition Manifest (PM) for a minimal Secure Partition (SP)
 * that has additional optional properties defined.
 *
 */

/dts-v1/;

/ {
	compatible = "arm,ffa-manifest-1.0";

	/* Properties */
	description = "op-tee";
	ffa-version = <0x00010000>; /* 31:16 - Major, 15:0 - Minor */
	uuid = <0x486178e0 0xe7f811e3 0xbc5e0002 0xa5d5c51b>;
	id = <1>;
	execution-ctx-count = <8>;
	exception-level = <2>; /* S-EL1 */
	execution-state = <0>; /* AARCH64 */
	load-address = <0x6280000>;
	entrypoint-offset = <0x1000>;
	xlat-granule = <0>; /* 4KiB */
	boot-order = <0>;
	messaging-method = <3>; /* Direct messaging only */
	run-time-model = <1>; /* Run to completion */

	/* Boot protocol */
	gp-register-num = <0x0>;

	device-regions {
		compatible = "arm,ffa-manifest-device-regions";

		uart1 {
			base-address = <0x00000000 0x1c0a0000>;
			pages-count = <1>;
			attributes = <0x3>; /* read-write */
		};

		gicd {
			base-address = <0x00000000 0x2f000000>;
			pages-count = <16>;
			attributes = <0x3>; /* read-write */
		};
	};
};
